**Project Proposal**

**CSEL-3208: Computer Peripheral & Interfacing Project (IOT)**

Presented by- **“Team Prefetch”**

**Name: Nishat Mahmud Name: Md. Waliul Islam Rayhan**

**ID: B190305003 ID: B190305034**

**Project title**: Portable Ultrasonic Range Meter for Non-Contact Distance Measurement.


**Problem statement**: Accurate and portable distance measurement is essential in various applications, such as robotics, industrial automation, and environmental monitoring. This project addresses the need for a cost-effective and portable solution for non-contact distance measurement.

**Objective**: The objective of this project is to design and implement a Portable Ultrasonic Range Meter based on Arduino and an Ultrasonic Sensor (HC-SR04). The system should be capable of accurately measuring distances in a non-contact fashion and displaying the results on a 16x2 LCD display. The primary goals include:

* Develop a compact and portable distance measurement device.
* Implement a user-friendly interface for real-time distance display.
* Achieve precise distance measurements with a range of 2cm to 400cm.
* Ensure low power consumption for extended battery life.
* Utilize the Arduino platform for ease of development and versatility.

**Features**: The Portable Ultrasonic Range Meter project offers the following key features:

* Non-contact distance measurement using ultrasonic technology.
* Accurate measurements within the range of 2cm to 400cm.
* Real-time distance display on a 16x2 LCD screen.
* Compact and portable design, suitable for various applications.
* Low power consumption, allowing the use of a 9V battery.
* User-adjustable contrast control for the LCD display.
* Continuous distance measurement without delays.
* Easy-to-use interface for versatile applications.

**Workflow diagram**:

**Fig:2 Flow Chart of Portable Ultrasonic Range Meter for Non-Contact Distance Measurement.**

**Tools and devices**:

* Arduino Uno microcontroller.
* Ultrasonic Sensor HC-SR04.
* 16x2 LCD Display.
* 10KΩ Potentiometer (POT).
* Breadboard and connecting wires.
* 9V battery or external power source.
* Connecting Wires
* Breadboard

**References**:

* "[Ultrasonic sensor based distance measurement](https://create.arduino.cc/projecthub/UnO/ultrasonic-sensor-based-distance-measurement-using-arduino-701947)" - Arduino Project Hub
* "[HC-SR04 Ultrasonic Sensor User Guide](https://www.electroschematics.com/hc-sr04-datasheet/)" – ElectroSchematics
* "[Arduino Official Website](https://www.arduino.cc/)" – Arduino
* "[Introduction to SONAR Technology](https://www.britannica.com/technology/sonar)" – Britannica